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HF R 75

HF - radial fan direct driven

Corrosion- resistant plastic radial fan, single inlet, housing in flame retarding PPs-el, injection- moulded and tight welded version, with sealing and grease-barrier on the shaft passage. Impeller in electrical- conductive PPs-el with vanes mounted on the back of the impeller for relief on shaft passage. All parts exposed to exhaust air are made of plastic or encapsulated by plastic. Motor encapsulated against the medium, with overload protection over the entire power range. Fan frame made of powder- coated steel sheet for mounting on horizontal ground.


Manufacturer	 			:  Hürner Luft- und Umwelttechnik
Type	 				:  HF R 75-16 D / … 
Housing-material	 		:  PPs-el
Impeller-material		 	:  PPs-el
Housing position	 		:  GL …
Inlet diameter	 			:  …	mm
Medium				:  air
Volume flow	 			:  ...	m³/h
Total pressure difference		:  …	Pa
Static pressure difference 		:  …	Pa
Sound pressure level Lp2A (1 m)	:  …	dB(A)
SFP (specific fan power)	 	:  … 	W/(m³/s)
Shaft power	 			:  …	kW
Motor power	 			:  …	kW
Voltage	 				:  …	V
Frequency	 			:  50	Hz
Rated current	 			:  …	A
Enclosure/motor protection	 	:  IP 55/…
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