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HF D … - 15 / 17 D

HF - radial roof fan

Corrosion resistant plastic radial roof fan with housing in stable, rotationally sintered version, one suction side, with splinter protection according to accident prevention rules from size 160 as plastic coated wire mesh. In case of upright mounting the exhaust air is blown out vertical according to requirements for aggressive air.All parts exposed to exhaust air made of plastic or encapsulated by plastic. Impeller with backward curved blades in injection moulded version, mounted with taper lock-bush on motor shaft, statically and  dynamically balanced, quality of balancing at least G 6.3 (DIN ISO 21940-11).
Including internally mounted motor, encapsulated against the delivery medium, and outside mounted repair switch in case of standard motors (without ex-protection) respectively externally mounted terminal box for ex-motors. External ventilation for the motor via outward located ducts.


Manufacturer	 			:  Hürner Luft- und Umwelttechnik
Type	 				:  HF D … - .. D 
Housing-material	 		:  PEs
Impeller-material		 	:  PPs
Inlet diameter	 			:  …	mm
Installation Position			: …
Medium				:  air
Volume flow	 			:  ...	m³/h
Total pressure difference		:  …	Pa
Static pressure difference 		:  …	Pa
Sound pressure level Lp2A (1 m)	:  …	dB(A)
SFP (specific fan power)	 	:  … 	W/(m³/s)

Motor power	 			:  …	kW
Voltage	 				:  …	V
Frequency	 			:  50	Hz
Rated current	 			:  …	A
Enclosure/motor protection	 	:  IP 55/ Kaltleiter
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