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HF D … - 16 D 

HF - radial roof fan

Corrosion resistant plastic radial roof fan with housing in thermoplastics, in stable, deep-drawn version, one inlet side, splinter protection according to accident prevention rules as plastic coated wire mesh. In case of upright mounting the exhaust air is blown out vertical according to requirements for aggressive air. All parts exposed to exhaust air are made of plastic or encapsulated by plastic. Shaft passage brought to minimum clearance using felt ring seal. Impeller with backward curved blades, floating-mounted on the motor shaft, statically and dynamically balanced, quality of balancing at least G 6.3 (DIN ISO 21940-11). Including internally mounted motor,encapsulated against the delivery medium, and outside mounted repair switch in case of standard motors (without ex-protection)respectively externally mounted terminal box for ex-motors. External ventilation for the motor via outward located ducts.


Manufacturer	 			:  Hürner Luft- und Umwelttechnik
Type	 				:  HF D … - 16 D 
Housing-material	 		:  PPs
Impeller-material		 	:  PPs
Inlet diameter	 			:  …	mm
Installation Position			: …
Medium				:  air
Volume flow	 			:  ...	m³/h
Total pressure difference		:  …	Pa
Static pressure difference 		:  …	Pa
Sound pressure level Lp2A (1 m)	:  …	dB(A)
SFP (specific fan power)	 	:  … 	W/(m³/s)

Motor power	 			:  …	kW
Voltage	 				:  …	V
Frequency	 			:  50	Hz
Rated current	 			:  …	A
Enclosure/motor protection	 	:  IP 55/ Kaltleiter
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